**Step 1:** While you wait for the file to download to your computer’s hard drive, insert the empty USB storage drive into your computer’s USB port.  
If your download didn’t begin automatically, click here to start the download again.

**Step 2:** Once the download is complete, locate the EA5T-14D544-AD.zip\* file that should now be saved to your computer’s hard drive.  
• You may need to navigate manually to the location to which you saved the file during Step 2 “Download Package”. (ex. ”Desktop”)

**TIP:** If you did not specify a location in Step 2, check for the .zip file in your computer’s “Downloads” or “My documents” folder. The file may have been saved to one of those folders by default.

**Step 3:** Double-click the .zip file to unzip and open it.  
If your computer has a third party extraction program such as WinZip, 7-Zip or WinRAR, you can also use that option to unzip and extract your file. For more information on how to unzip and extract files using one of these programs, see the corresponding third party developer’s website.

**Step 4:** Select all of the items inside the unzipped folder. Drag and drop them onto your USB drive.  
**NOTE:** Installing the software update files in your vehicle will only work if the SyncMyRide and additional file(s)\* are visible on the USB drive. Do not combine or delete any of the files.

**Step 5:** Select your USB Drive to view Its contents and ensure that the correct folder and files are listed.

**Step 6:** Right-click on your USB drive and choose “Eject” to safely eject the USB drive from your computer.